<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<packages>
<package name="SSOP16">
<description>SSOP-16, 0.32 x 1.26 mm pad, 0.63mm pitch, 6.82mm Pad length</description>
</package>
<package name="FB1206">
</package>
<package name="FB402">
</package>
<package name="FB805">
</package>
<package name="FB603">
</package>
<package name="C805">
</package>
<package name="C603">
</package>
<package name="C1206">
</package>
<package name="SMC_A">
</package>
<package name="SMC_B">
</package>
<package name="CASE_A">
</package>
<package name="CASE_B">
</package>
<package name="PH-1X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="PH-1X05/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="R805">
</package>
<package name="R603">
</package>
<package name="R402">
</package>
<package name="R1206">
</package>
<package name="CON-USB-A-M">
<description>SMD mount USB Type A Male</description>
</package>
<package name="L1206">
</package>
<package name="L805">
</package>
<package name="L603">
</package>
</packages>
<symbols>
<symbol name="FT230X">
<pin name="3V3OUT" direction="pwr"/>
<pin name="USB-" direction="in"/>
<pin name="USB+" direction="out"/>
<pin name="!RESET"/>
<pin name="GND@1" direction="sup"/>
<pin name="GND@2" direction="sup"/>
<pin name="CBUS3"/>
<pin name="CBUS2"/>
<pin name="CBUS1"/>
<pin name="CBUS0"/>
<pin name="!CTS"/>
<pin name="!RTS"/>
<pin name="RXD" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="VCC" direction="sup"/>
<pin name="VCCIO" direction="pwr"/>
</symbol>
<symbol name="INDUCTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CAPACITOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CAPACITOR-POL">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
<symbol name="PIN-HD-5">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
</symbol>
<symbol name="RESISTOR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="+3V3">
<pin name="+3V3" direction="sup"/>
</symbol>
<symbol name="+5V">
<pin name="+5V" direction="sup"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="CON-USB">
<pin name="GND"/>
<pin name="VUSB"/>
<pin name="D-"/>
<pin name="D+"/>
</symbol>
<symbol name="USB-BODY-PINS">
<pin name="BODY@4" direction="hiz"/>
<pin name="BODY@3" direction="hiz"/>
<pin name="BODY@1" direction="hiz"/>
<pin name="BODY@2" direction="hiz"/>
</symbol>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="FTDI-FT230X" prefix="IC">
<description>BASIC USB to UART IC</description>
<gates>
<gate name="IC" symbol="FT230X"/>
</gates>
<devices>
<device name="-SSOP-16" package="SSOP16">
<connects>
<connect gate="IC" pin="!CTS" pad="6"/>
<connect gate="IC" pin="!RESET" pad="11"/>
<connect gate="IC" pin="!RTS" pad="2"/>
<connect gate="IC" pin="3V3OUT" pad="10"/>
<connect gate="IC" pin="CBUS0" pad="15"/>
<connect gate="IC" pin="CBUS1" pad="14"/>
<connect gate="IC" pin="CBUS2" pad="7"/>
<connect gate="IC" pin="CBUS3" pad="16"/>
<connect gate="IC" pin="GND@1" pad="5"/>
<connect gate="IC" pin="GND@2" pad="13"/>
<connect gate="IC" pin="RXD" pad="4"/>
<connect gate="IC" pin="TXD" pad="1"/>
<connect gate="IC" pin="USB+" pad="8"/>
<connect gate="IC" pin="USB-" pad="9"/>
<connect gate="IC" pin="VCC" pad="12"/>
<connect gate="IC" pin="VCCIO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FERRITE-BEAD" prefix="L" uservalue="yes">
<description>Ferrite bead in various packages</description>
<gates>
<gate name="L" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="-1206" package="FB1206">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0805" package="FB805">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0603" package="FB603">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C" prefix="C" uservalue="yes">
<description>Non-Polarized capacitor in various packages</description>
<gates>
<gate name="C" symbol="CAPACITOR"/>
</gates>
<devices>
<device name="-0805" package="C805">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0603" package="C603">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-1206" package="C1206">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C-POL" prefix="C" uservalue="yes">
<description>Polarized capacitor in various packages</description>
<gates>
<gate name="C" symbol="CAPACITOR-POL"/>
</gates>
<devices>
<device name="-SMC_A" package="SMC_A">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMC_B" package="SMC_B">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CASE_A" package="CASE_A">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CASE_B" package="CASE_B">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-PINHD-1X5" prefix="JP" uservalue="yes">
<description>Pin header 1x05</description>
<gates>
<gate name="A" symbol="PIN-HD-5"/>
</gates>
<devices>
<device name="" package="PH-1X05">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="PH-1X05/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R" prefix="R" uservalue="yes">
<description>Resistor in various packages</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="-0805" package="R805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0603" package="R603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+3V3" prefix="+3V3">
<description>Power supply +3.3V</description>
<gates>
<gate name="G$1" symbol="+3V3"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+5V" prefix="+5V">
<description>Power supply +5V</description>
<gates>
<gate name="SUPPLY" symbol="+5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND" prefix="GND">
<description>Supply GND</description>
<gates>
<gate name="G$1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-USB" prefix="USB" uservalue="yes">
<description>USB Male connector</description>
<gates>
<gate name="USB" symbol="CON-USB"/>
<gate name="BODY" symbol="USB-BODY-PINS"/>
</gates>
<devices>
<device name="-A" package="CON-USB-A-M">
<connects>
<connect gate="BODY" pin="BODY@1" pad="BODY@1"/>
<connect gate="BODY" pin="BODY@2" pad="BODY@2"/>
<connect gate="BODY" pin="BODY@3" pad="BODY@3"/>
<connect gate="BODY" pin="BODY@4" pad="BODY@4"/>
<connect gate="USB" pin="D+" pad="D+"/>
<connect gate="USB" pin="D-" pad="D-"/>
<connect gate="USB" pin="GND" pad="GND"/>
<connect gate="USB" pin="VUSB" pad="VUSB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" prefix="LED" uservalue="yes">
<description>LED</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="L0805" package="L805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L0603" package="L603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L1206" package="L1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
